NOTES:
	2-		Use two Torx bits (item 60), to align the field with the field case. Gently tap field case on rigid surface so that field slides into field case.
	8-		Press flush with end of shaft; seal to face commutator.
	9-		End of shaft to bearing 1.048"-1.052"; seal to face fan.
	29-		Date Code: Located on bottom of field case.
	42-		Left hand thread. 5-7 in./lb. torque.

LUBRICATION:
Distribute 84-86 grams of BD L2.0 grease in gear case.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.