R11483
D25111, D25112, D25113, D25114, D25213, D25314, D25315, DWC24K3.
Item No.

50	The Inter shaft is only available as a SA.

77		A camisa do pistão é diferente do sistema anterior.
		O furo da camisa (77) é requerido já não é requerido, o pistão tem que ser pressionado na 			camisa com alguma força até que o anel-O (76) agarre no sulco interno no pistão.
								
90	Avoid damage to the cylinder (114) wall when removing / refitting the snap ring.

112	The clutch is only available as a SA.

114		The Spindle is only available as a SA.

160	The side handle is only available as a SA.

836	Service tool is required to release (items 6, 10, 11) from the connector (item 9) 
D25313 & D25314 ONLY.

846	The Service kit includes  all O Rings, Seals, Brushes, Screws and Grease ( items 5,45, 51, 55, 60, 62x2, 72, 76, 79x3, 92, 93x2, 97, 136, 800, 801) .  Item 45 O Ring is not required when repairing units with the QCC system.

Lubrication.

800		Paragon Grease.
30grms inside the Housing (70) around the hollow piston and Wobble Bearing. 
20grms over the Clutch (112) and inter gear (50).
1.2grms spread over (items 91, 92, 93, 94, 95, 96).
0.5grm around the Steel Ball (134) and the tool holder end of Cylinder (114).

801		GLK Grease.
2grms on the inside of Cylinder (114).
1grm over the Ram (77) and O Ring (76).
2grms spread between inside & outside of the Hollow Piston (75).
1.2grms on the pivot bolt (73) & Washers (74).
1.0grms on the Intershaft (50) Finger. 

Touque Settings.

9		2.0 Nm
22		2.6 Nm
23	1.0 Nm Field x 2.
23		0.6 Nm Fan Baffel  x 2.
35	1.5 Nm 
37		1.5 Nm
40		1.0 Nm
57	1.5 Nm
62	3.2 Nm
79	3.2 Nm
116	2.0 Nm
121		1.8 Nm