R10055

Cat no MSS810E type 1, P5321 Cut-Saw

When fitting the ball bearing, item 9, to the armature shaft, make sure the seal faces the commutator. Press the bearing flush with the end of the shaft.

When fitting the ball bearing, item 10, to the armature shaft, make sure the seal faces the fan. The bearing should be pressed on the shaft so that the distance from the end of the shaft to the outside face of the bearing is between 26.6 mm and 26.7 mm.

Lubrication.
Distribute 17 gms of grease in the gear case and fill the depressed circular area of the cover plate with grease.

The date code of the unit can be found on the bottom of the fieldcase, item 43.

Item 28, shoe.
Users who have the pipe cutting attachment E35400, which was made before December 1995, must use the shoe, item 28, date up to 5295.

Users who have the pipe cutting attachment E35400, which was made after December 1995, must use the shoe, item 28, date from 5295.

The Powered Metal Gear, Item 34, has been replaced by a Machined Metal Gear form Date code 9910.