R10029

MSS810E and MSS81E - Type 100    -     Cut Saw.

When replacing the shaft, item 29, it is recommended to also replace the bearing, item 32.

Item 9:	 Bearing seal faces commutator and press flush with the end of the shaft.

Item 10, bearing, seal faces fan with end shaft to bearing 26.6 mm, 26.7 mm.

Date code is located on the bottom of the field case, item 43.

Lubricate with 17 gms of grease in gear case and fill depressed circular plate with grease.

Item 28, shoe.
Users who have the pipe cutting attachment E35400, which was made before December 1995, must use the shoe, item 28, date up to 5295.

Users who have the pipe cutting attachment E35400, which was made after December 1995, must use the shoe, item 28, date from 5295.

Item 29 shaft sa includes items 23 rollpin and 27 pin.
Item 30 blade clamp sa includes items 21 screw,  23 rollpin and 27 pin.
Item 33 crank bearing sa includes an instruction sheet.

Item 34, The Powered Metal Gear has been replaced by a Machined Metal Gear from Date code 9910