R10013
MH85 CIRCULAR SAW

RESISTANCE VALUES IN OHMS:

Armature 115 / 120 =		0.5
Armature 220 / 240 =		1.5
Field 115 / 120 =		0.4 per winding
Field 220 / 240 =		0.7 per winding